
SYMMETRON VERIVANE

Installation instructions:

**********************************************************************************************************************************************

Á) If you are installing the VeriVane software for the first time:

1. Install the usb drivers, by running the CDM20814_Setup.exe file which is located in the 'VeriVanePackage_Version_2.2.0.0' folder.

2. Copy the 'VeriVane_Version_2.0.0' folder from the 'VeriVanePackage_Version_2.2.0.0' folder in your computer's 'C:\' folder.

3. Open a command line (command prompt) as Administrator, from 'Start-->Programs-->Accessories'. Right-click 'Command Line' and select "Run as 
Administrator".

4. According to your operating system version:

	É. 32-BIT WINDOWS 
		- Copy the 'PolarCryptoLight.dll' file from the 'VeriVanePackage_Version_2.2.0.0' folder to 'C:\WINDOWS\SYSTEM32\'
		- In the opened command line, type: 
			CD C:\WINDOWS\SYSTEM32\
		and press ENTER.

		- Type:
 			Regsvr32 polarcryptolight.dll
		and wait for a message that it is successfully installed.

	ÉÉ. 64-ÂÉÔ WINDOWS
		- Copy the 'PolarCryptoLight.dll' from the 'VeriVanePackage_Version_2.2.0.0' folder to 'C:\WINDOWS\SYSWOW64\'
		- In the opened command line, type: 
			CD C:\WINDOWS\SYSWOW64\
		and press ENTER.

		- Type:
 			Regsvr32 polarcryptolight.dll
		and wait for a message that it is successfully installed.

5. Open the 'VeriVaneExe' folder in the 'VeriVanePackage_Version_2.2.0.0' and install the program (setup.exe).

6. After installation, the program is located in 'Start-->Programs-->Symmetron-->VeriVane'.

---------------------------------------------------------------------------------------------------------------------------------------------------

Note 1: When you have connected the instrument's (VeriVane) USB cable to a computer port, go to Control Panel-->System. In the 'Hardware' tab, 
	select 'Device Manager' and then select 'COM&LPT ports'. From the appearing list, select the USB Serial Port(COMx), where x is a number.
	In the appearing window, open the 'Port Settings' and select the following settings (even if they appear already selected), by clicking them: 

		Bits per second:9600
		Data bits:8
		Parity:None
		Stop bits:1
		Flow control:None

	and press OK.

***************************************************************************************************************************************************

Â) If you have installed a previous Version of the VeriVane software:

1. Uninstall the VeriVane software from Control Panel-->Add/Remove Programs. Select the VeriVane program and select 'Remove'.
2. Copy the 'VeriVane_Version_2.0.0' folder from 'VeriVanePackage_Version_2.2.0.0' in your computer's C:\ folder.
3. Open the 'VeriVaneExe' folder in the 'VeriVanePackage_Version_2.2.0.0' and install the program (setup.exe).
4. After installation, the program is located in 'Start-->Programs-->Symmetron-->VeriVane'.

***************************************************************************************************************************************************

For more information, contact us:

Tel: +30-2106034002
Fax: +30-2106034003
email: support@symmetron.gr
www.symmetron.gr



